(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu16.04.1)

  (general
    (thickness 1.6)
    (drawings 30)
    (tracks 39)
    (zones 0)
    (modules 10)
    (nets 8)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00040_7ffffffe)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 3)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 "Net-(C25-Pad1)")
  (net 2 "Net-(C25-Pad2)")
  (net 3 "Net-(D5-Pad1)")
  (net 4 "Net-(D5-Pad2)")
  (net 5 "Net-(F1-Pad2)")
  (net 6 "Net-(F1-Pad1)")
  (net 7 "Net-(J1-Pad2)")

  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C25-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J1-Pad2)")
  )

  (module Capacitor_THT:C_Disc_D14.5mm_W5.0mm_P10.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5D44471D)
    (at 35.83 19.32 90)
    (descr "C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=14.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 10.00mm  diameter 14.5mm width 5.0mm Capacitor")
    (path /5BCEF457)
    (fp_text reference C25 (at 5 -3.75 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "203M SF 250V AC" (at 5 3.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.25 -2.5) (end -2.25 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.25 2.5) (end 12.25 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 12.25 2.5) (end 12.25 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 12.25 -2.5) (end -2.25 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.37 -2.62) (end 12.37 -2.62) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.37 2.62) (end 12.37 2.62) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.37 -2.62) (end -2.37 2.62) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.37 -2.62) (end 12.37 2.62) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.5 -2.75) (end -2.5 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 2.75) (end 12.5 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.5 2.75) (end 12.5 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.5 -2.75) (end -2.5 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 5 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C25-Pad1)"))
    (pad 2 thru_hole circle (at 10 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C25-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D14.5mm_W5.0mm_P10.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module mixersupply_fuse:Fuseholder0520 (layer F.Cu) (tedit 5BC4A14C) (tstamp 5D444CEB)
    (at 30.173639 33.02)
    (path /5BA8F401)
    (fp_text reference F1 (at 6.656361 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Fuse 1.6A T" (at 0 -6.35) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 13.97 -3.81) (end 13.97 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 13.97 3.81) (end -13.97 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -13.97 3.81) (end -13.97 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -13.97 -3.81) (end 13.97 -3.81) (layer F.SilkS) (width 0.15))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 4.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(F1-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 4.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(F1-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0 90) (size 4.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 6 "Net-(F1-Pad1)"))
    (pad 1 thru_hole oval (at -10.16 0 90) (size 4.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 6 "Net-(F1-Pad1)"))
  )

  (module mixersupply_connectors:AC_Connector (layer F.Cu) (tedit 5D4449A4) (tstamp 5D444500)
    (at 5.35 20.59 90)
    (path /5BAE5D12)
    (fp_text reference J1 (at 0 -6.985 90) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "230V In" (at 0 -8.255 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -10.16 -3.5) (end 10.16 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 10.16 -3.5) (end 10.16 3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 10.16 3.5) (end -10.16 3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -10.16 3.5) (end -10.16 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -3.556) (end 1.524 -3.556) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 -3.556) (end 1.524 3.556) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 3.556) (end -1.524 3.556) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.524 3.556) (end -1.524 -3.556) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.524 -3.556) (end 0 -3.556) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 6 6) (drill 2) (layers *.Cu *.Mask)
      (net 6 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 6 6) (drill 2) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
  )

  (module mixersupply_connectors:2Pin_8mm_w_clipconnector (layer F.Cu) (tedit 5D444941) (tstamp 5CEFA622)
    (at 53.15 33.02 180)
    (path /5BD2B533)
    (fp_text reference J2 (at 0 -6.35 180) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "PWR Switch" (at 0 -7.62 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 6.35 -3.81) (end 6.35 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 6.35 3.81) (end -6.35 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -6.35 3.81) (end -6.35 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -6.35 -3.81) (end -5.08 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -3.81) (end -5.08 -5.08) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -5.08) (end 5.08 -5.08) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -5.08) (end 5.08 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -3.81) (end 6.35 -3.81) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole oval (at 4 0 270) (size 4.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(F1-Pad2)"))
    (pad 2 thru_hole oval (at -4 0 270) (size 4.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "Net-(C25-Pad1)"))
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5D444ADC) (tstamp 5D444A5E)
    (at 81.28 21.59 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (path /5CF08DB4)
    (fp_text reference J3 (at 0 -2.33 180) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Relais_on (at 0 4.87 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module mixersupply_connectors:2Pin_8mm_w_clipconnector (layer F.Cu) (tedit 5D44493A) (tstamp 5D4446EB)
    (at 23.13 9.16)
    (path /5BC67AD5)
    (fp_text reference J6 (at 0 -6.35) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Transformator Primary" (at 0 -7.62) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5.08 -3.81) (end 6.35 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -5.08) (end 5.08 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -5.08) (end 5.08 -5.08) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -3.81) (end -5.08 -5.08) (layer F.SilkS) (width 0.15))
    (fp_line (start -6.35 -3.81) (end -5.08 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -6.35 3.81) (end -6.35 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 6.35 3.81) (end -6.35 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 6.35 -3.81) (end 6.35 3.81) (layer F.SilkS) (width 0.15))
    (pad 2 thru_hole oval (at -4 0 90) (size 4.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 1 thru_hole oval (at 4 0 90) (size 4.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(C25-Pad2)"))
  )

  (module "mixersupply_relay:Relais DEG SDT-S-105LMR" (layer F.Cu) (tedit 5BC4BB47) (tstamp 5D444B19)
    (at 74.93 24.13 180)
    (path /5BD04C3D)
    (fp_text reference K1 (at 0 -10.16 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "DEG SDT-S-105LMR" (at 0 -11.43 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.81 -2.54) (end 24.13 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 24.13 -2.54) (end 24.13 10.16) (layer F.SilkS) (width 0.15))
    (fp_line (start 24.13 10.16) (end -3.81 10.16) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.81 10.16) (end -3.81 -2.54) (layer F.SilkS) (width 0.15))
    (pad A1 thru_hole circle (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D5-Pad1)"))
    (pad A2 thru_hole circle (at 0 7.62 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D5-Pad2)"))
    (pad 11 thru_hole circle (at 16.51 7.62 180) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(C25-Pad2)"))
    (pad 14 thru_hole circle (at 20.32 0 180) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C25-Pad1)"))
  )

  (module Varistor:RV_Disc_D7mm_W3.4mm_P5mm (layer F.Cu) (tedit 5A0F68DF) (tstamp 5D444678)
    (at 25.67 19.32 180)
    (descr "Varistor, diameter 7mm, width 3.4mm, pitch 5mm")
    (tags "varistor SIOV")
    (path /5BDC383D)
    (fp_text reference RV1 (at 2.5 3.35 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Varistor (at 2.5 -2.05 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0.65 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.25 2.6) (end 6.25 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -1.3) (end 6.25 -1.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.25 -1.3) (end 6.25 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -1.3) (end -1.25 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 2.35) (end 6 2.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 -1.05) (end 6 -1.05) (layer F.SilkS) (width 0.15))
    (fp_line (start 6 -1.05) (end 6 2.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 -1.05) (end -1 2.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 2.35) (end 6 2.35) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -1.05) (end 6 -1.05) (layer F.Fab) (width 0.1))
    (fp_line (start 6 -1.05) (end 6 2.35) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -1.05) (end -1 2.35) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(C25-Pad1)"))
    (pad 2 thru_hole circle (at 5 1.3 180) (size 1.6 1.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Varistor.3dshapes/RV_Disc_D7mm_W3.4mm_P5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Varistor:RV_Disc_D21.5mm_W4.8mm_P10mm (layer F.Cu) (tedit 5A0F68FE) (tstamp 5D4446AE)
    (at 41.5 19.16 90)
    (descr "Varistor, diameter 21.5mm, width 4.8mm, pitch 10mm")
    (tags "varistor SIOV")
    (path /5BCBFCA3)
    (fp_text reference TH1 (at 5 4.375 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Thermistor_NTC (at 5 -2.425 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 5 0.975 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -6 3.63) (end 16 3.63) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6 -1.68) (end 16 -1.68) (layer F.CrtYd) (width 0.05))
    (fp_line (start 16 -1.68) (end 16 3.63) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6 -1.68) (end -6 3.63) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.75 3.375) (end 15.75 3.375) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.75 -1.425) (end 15.75 -1.425) (layer F.SilkS) (width 0.15))
    (fp_line (start 15.75 -1.425) (end 15.75 3.375) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.75 -1.425) (end -5.75 3.375) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.75 3.375) (end 15.75 3.375) (layer F.Fab) (width 0.1))
    (fp_line (start -5.75 -1.425) (end 15.75 -1.425) (layer F.Fab) (width 0.1))
    (fp_line (start 15.75 -1.425) (end 15.75 3.375) (layer F.Fab) (width 0.1))
    (fp_line (start -5.75 -1.425) (end -5.75 3.375) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C25-Pad1)"))
    (pad 2 thru_hole circle (at 10 1.95 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C25-Pad2)"))
    (model ${KISYS3DMOD}/Varistor.3dshapes/RV_Disc_D21.5mm_W4.8mm_P10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_SMD:D_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer B.Cu) (tedit 5B4B45C8) (tstamp 5D444FA2)
    (at 74.93 20.0125 90)
    (descr "Diode SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (path /5BA90880)
    (attr smd)
    (fp_text reference D5 (at 0 2.28 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value DIODE (at 0 -2.28 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.6 1.25) (end -0.975 1.25) (layer B.Fab) (width 0.1))
    (fp_line (start -0.975 1.25) (end -1.6 0.625) (layer B.Fab) (width 0.1))
    (fp_line (start -1.6 0.625) (end -1.6 -1.25) (layer B.Fab) (width 0.1))
    (fp_line (start -1.6 -1.25) (end 1.6 -1.25) (layer B.Fab) (width 0.1))
    (fp_line (start 1.6 -1.25) (end 1.6 1.25) (layer B.Fab) (width 0.1))
    (fp_line (start 1.6 1.585) (end -2.46 1.585) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.46 1.585) (end -2.46 -1.585) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.46 -1.585) (end 1.6 -1.585) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.45 -1.58) (end -2.45 1.58) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.45 1.58) (end 2.45 1.58) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.45 1.58) (end 2.45 -1.58) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.45 -1.58) (end -2.45 -1.58) (layer B.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)) (justify mirror))
    )
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 2.65) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 3 "Net-(D5-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 2.65) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text "For plastic case:\nKunststoffgehäuse 0021-002-093\n95x48x37 (outer dimensions)" (at 30.48 46.99) (layer F.Fab)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Relais\non" (at 81.28 27.94 90) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Trafo Primary" (at 22.86 2.54) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Mains in" (at 12.7 20.32 90) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text T1.6A (at 30.48 25.4) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text Switch (at 64.77 36.83) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 29.21 38.1) (end 29.21 27.94) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 31.75 38.1) (end 29.21 38.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 31.75 27.94) (end 31.75 38.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 29.21 27.94) (end 31.75 27.94) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 7 34) (end 0 34) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 10.43 21.86) (end 0.27 21.86) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 7 41) (end 7 34) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 66.31 29.575) (end 63.77 29.575) (layer Edge.Cuts) (width 0.1) (tstamp 5D444A47))
  (gr_line (start 7 7) (end 7 0) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0 7) (end 7 7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79 34) (end 79 41) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 86 34) (end 79 34) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79 7) (end 86 7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79 0) (end 79 7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.27 21.86) (end 0.27 19.32) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 10.43 19.32) (end 10.43 21.86) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.27 19.32) (end 10.43 19.32) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0 34) (end 0 7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79 41) (end 7 41) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 86 7) (end 86 34) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 7 0) (end 79 0) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.77 11.795) (end 63.77 29.575) (layer Edge.Cuts) (width 0.1) (tstamp 5D444A44))
  (gr_line (start 66.31 11.795) (end 63.77 11.795) (layer Edge.Cuts) (width 0.1) (tstamp 5D444A41))
  (gr_line (start 66.31 29.575) (end 66.31 11.795) (layer Edge.Cuts) (width 0.1) (tstamp 5D444A3E))

  (via (at 11.75 11.5) (size 5) (drill 3) (layers F.Cu B.Cu) (net 0))
  (via (at 74.25 11.5) (size 5) (drill 3) (layers F.Cu B.Cu) (net 0) (tstamp 5CEFB6A1))
  (via (at 74.25 29.5) (size 5) (drill 3) (layers F.Cu B.Cu) (net 0) (tstamp 5CEFB6A3))
  (via (at 11.75 29.5) (size 5) (drill 3) (layers F.Cu B.Cu) (net 0) (tstamp 5CEFB3E8))
  (segment (start 35.83 19.32) (end 25.67 19.32) (width 2) (layer B.Cu) (net 1) (tstamp 5D444709) (status 30))
  (segment (start 35.99 19.16) (end 35.83 19.32) (width 2) (layer B.Cu) (net 1) (tstamp 5D444661) (status 30))
  (segment (start 41.5 19.16) (end 35.99 19.16) (width 2) (layer B.Cu) (net 1) (tstamp 5D44465E) (status 30))
  (segment (start 57.15 26.67) (end 54.61 24.13) (width 2) (layer B.Cu) (net 1))
  (segment (start 57.15 33.02) (end 57.15 26.67) (width 2) (layer B.Cu) (net 1))
  (segment (start 41.5 19.16) (end 45.83 19.16) (width 2) (layer B.Cu) (net 1))
  (segment (start 45.83 19.16) (end 50.8 24.13) (width 2) (layer B.Cu) (net 1))
  (segment (start 50.8 24.13) (end 54.61 24.13) (width 2) (layer B.Cu) (net 1))
  (segment (start 35.99 9.16) (end 35.83 9.32) (width 2) (layer B.Cu) (net 2) (tstamp 5D4446D6) (status 30))
  (segment (start 43.45 9.16) (end 35.99 9.16) (width 2) (layer B.Cu) (net 2) (tstamp 5D4446D3) (status 30))
  (segment (start 35.67 9.16) (end 35.83 9.32) (width 2) (layer B.Cu) (net 2) (tstamp 5D44465B))
  (segment (start 27.13 9.16) (end 35.67 9.16) (width 2) (layer B.Cu) (net 2) (tstamp 5D444664))
  (segment (start 51.07 9.16) (end 43.45 9.16) (width 2) (layer B.Cu) (net 2))
  (segment (start 58.42 16.51) (end 51.07 9.16) (width 2) (layer B.Cu) (net 2))
  (segment (start 74.93 24.13) (end 74.93 21.5) (width 1) (layer B.Cu) (net 3))
  (segment (start 81.28 22.94) (end 80.09 24.13) (width 1) (layer B.Cu) (net 3))
  (segment (start 81.28 21.59) (end 81.28 22.94) (width 1) (layer B.Cu) (net 3))
  (segment (start 80.09 24.13) (end 74.93 24.13) (width 1) (layer B.Cu) (net 3))
  (segment (start 74.93 16.51) (end 74.93 18.525) (width 1) (layer B.Cu) (net 4))
  (segment (start 81.28 19.05) (end 81.28 17.78) (width 1) (layer B.Cu) (net 4))
  (segment (start 80.01 16.51) (end 74.93 16.51) (width 1) (layer B.Cu) (net 4))
  (segment (start 81.28 17.78) (end 80.01 16.51) (width 1) (layer B.Cu) (net 4))
  (segment (start 35.253639 33.02) (end 40.333639 33.02) (width 2) (layer B.Cu) (net 5))
  (segment (start 40.333639 33.02) (end 49.15 33.02) (width 2) (layer B.Cu) (net 5))
  (segment (start 5.35 25.67) (end 6.89 24.13) (width 2) (layer B.Cu) (net 6))
  (segment (start 6.89 24.13) (end 16.51 24.13) (width 2) (layer B.Cu) (net 6))
  (segment (start 20.013639 27.633639) (end 20.013639 33.02) (width 2) (layer B.Cu) (net 6))
  (segment (start 16.51 24.13) (end 20.013639 27.633639) (width 2) (layer B.Cu) (net 6))
  (segment (start 20.013639 33.02) (end 25.093639 33.02) (width 2) (layer B.Cu) (net 6))
  (segment (start 19.13 16.48) (end 20.67 18.02) (width 2) (layer B.Cu) (net 7) (tstamp 5D4446DC))
  (segment (start 19.13 9.16) (end 19.13 16.48) (width 2) (layer B.Cu) (net 7) (tstamp 5D4446D9))
  (segment (start 17.83 17.78) (end 19.13 16.48) (width 2) (layer B.Cu) (net 7))
  (segment (start 10.16 17.78) (end 17.83 17.78) (width 2) (layer B.Cu) (net 7))
  (segment (start 7.89 15.51) (end 10.16 17.78) (width 2) (layer B.Cu) (net 7))
  (segment (start 5.35 15.51) (end 7.89 15.51) (width 1) (layer B.Cu) (net 7))

)
