Cmp-Mod V01 Created by Cvpcb (2015-03-21 BZR 5528)-product   date = Thu 26 Mar 2015 02:44:40 PM EET

BeginCmp
TimeStamp = /54D21881;
Reference = C1;
ValeurCmp = 18p;
IdModule  = Capacitors_SMD:C_0603;
EndCmp

BeginCmp
TimeStamp = /54D218DE;
Reference = C2;
ValeurCmp = 18p;
IdModule  = Capacitors_SMD:C_0603;
EndCmp

BeginCmp
TimeStamp = /54D21E5C;
Reference = C3;
ValeurCmp = 1u;
IdModule  = Capacitors_SMD:C_0603;
EndCmp

BeginCmp
TimeStamp = /54D2222A;
Reference = C4;
ValeurCmp = 1n;
IdModule  = Capacitors_SMD:C_0603;
EndCmp

BeginCmp
TimeStamp = /54D22484;
Reference = C5;
ValeurCmp = 1n;
IdModule  = Capacitors_SMD:C_0603;
EndCmp

BeginCmp
TimeStamp = /54D2428C;
Reference = C6;
ValeurCmp = 1u;
IdModule  = Capacitors_SMD:C_0603;
EndCmp

BeginCmp
TimeStamp = /551427DB;
Reference = C7;
ValeurCmp = 1u;
IdModule  = Capacitors_SMD:C_0603;
EndCmp

BeginCmp
TimeStamp = /551434BC;
Reference = C8;
ValeurCmp = 1u;
IdModule  = Capacitors_SMD:C_0603;
EndCmp

BeginCmp
TimeStamp = /54D21FCD;
Reference = D1;
ValeurCmp = DIODESCH;
IdModule  = SMD_Packages:SOD-523;
EndCmp

BeginCmp
TimeStamp = /54D22068;
Reference = D2;
ValeurCmp = DIODESCH;
IdModule  = SMD_Packages:SOD-523;
EndCmp

BeginCmp
TimeStamp = /54D22B40;
Reference = P1;
ValeurCmp = CONN_01X06;
IdModule  = Pin_Headers:Pin_Header_Straight_2x03;
EndCmp

BeginCmp
TimeStamp = /54D22CB3;
Reference = Q1;
ValeurCmp = MOSFET_P;
IdModule  = SMD_Packages:SOT-23-GDS;
EndCmp

BeginCmp
TimeStamp = /54D2193D;
Reference = R1;
ValeurCmp = 1M;
IdModule  = Resistors_SMD:R_0603;
EndCmp

BeginCmp
TimeStamp = /5514275D;
Reference = R2;
ValeurCmp = 10k;
IdModule  = Resistors_SMD:R_0603;
EndCmp

BeginCmp
TimeStamp = /54D22EA4;
Reference = R3;
ValeurCmp = 1M;
IdModule  = Resistors_SMD:R_0603;
EndCmp

BeginCmp
TimeStamp = /54D2209D;
Reference = R4;
ValeurCmp = 330;
IdModule  = Resistors_SMD:R_0603;
EndCmp

BeginCmp
TimeStamp = /54D22174;
Reference = R5;
ValeurCmp = 1M;
IdModule  = Resistors_SMD:R_0603;
EndCmp

BeginCmp
TimeStamp = /54D2252C;
Reference = R6;
ValeurCmp = 1M;
IdModule  = Resistors_SMD:R_0603;
EndCmp

BeginCmp
TimeStamp = /54D222F8;
Reference = R7;
ValeurCmp = 1M;
IdModule  = Resistors_SMD:R_0603;
EndCmp

BeginCmp
TimeStamp = /54D221C8;
Reference = R8;
ValeurCmp = 1M;
IdModule  = Resistors_SMD:R_0603;
EndCmp

BeginCmp
TimeStamp = /54D2B12F;
Reference = R9;
ValeurCmp = 10k 0.1%;
IdModule  = Resistors_SMD:R_0603;
EndCmp

BeginCmp
TimeStamp = /54D2B156;
Reference = R10;
ValeurCmp = 10k 0.1%;
IdModule  = Resistors_SMD:R_0603;
EndCmp

BeginCmp
TimeStamp = /54D2B17D;
Reference = R11;
ValeurCmp = 10k 0.1%;
IdModule  = Resistors_SMD:R_0603;
EndCmp

BeginCmp
TimeStamp = /54D2B42B;
Reference = R12;
ValeurCmp = 10k 0.1%;
IdModule  = Resistors_SMD:R_0603;
EndCmp

BeginCmp
TimeStamp = /551426A3;
Reference = R13;
ValeurCmp = 330;
IdModule  = Resistors_SMD:R_0603;
EndCmp

BeginCmp
TimeStamp = /54D21739;
Reference = U1;
ValeurCmp = NC7WZU04P6;
IdModule  = Transistors_SMD:sc70-6;
EndCmp

BeginCmp
TimeStamp = /54D2AB47;
Reference = U2;
ValeurCmp = LM324;
IdModule  = Housings_SSOP:TSSOP-14_4.4x5mm_Pitch0.65mm;
EndCmp

BeginCmp
TimeStamp = /54D213EA;
Reference = X1;
ValeurCmp = 16MHz;
IdModule  = Crystals:Crystal_HC49-SD_SMD;
EndCmp

EndListe
